**Level Float Switch (1FLUTTI05P)**

* Rated Voltage: 240 Volt AC
* Max Current: (4) 10A
* Max Pressure: 1 Bar
* Protection Class: II
* Weight: 265g
* Material (float switch): Polypropylene (PP)
* Material (cable): PVC + Neoprene
* Operation Temperature: 0 – 60 Degrees C
* IP68
* 5m cable

